DS3231 Real-Time Clock Commands

The DS3231.h include file provides both high- and low-level support for the DS3231 real-time clock chip, two alarms with a backup battery, and two IO ports. Insert the following directive in your code to make these new commands available:

*#include < DS3231.h>*

Here follows a list of the commands..

DS3231\_EnableOscillator(flag)  
enables the clock when flag is TRUE,  
disables the clock when flag is FALSE

DS3231\_OscillatorStopFlagStatus  
A function that returns the status of the Oscillator.

DS3231\_ClearOscillatorStopFlag  
A method to clear the Oscillator stop flag. To be used after a power failure.

DS3231\_ResetClock  
resets clock completely to manufacturer’s original condition,  
time to 00:00:00, day of the week to 01, date to 01/01/00,  
also sets 24-hour mode and enables the clock.

DS3231\_SetClock(hour, minute, second, DOW, date, month, year)  
sets the entire clock: hours, minutes, seconds, day of week, date, month, year.  
there is no error detection for out-of-range dates, (e.g., April 31)  
also sets 24-hour mode and enables the clock.

DS3231\_SetTime(hour, minute, second)  
sets the time only: hours, minutes, seconds,.  
also sets 24-hour mode and enables the clock.

DS3231\_SetDate(dayoftheweek, date, month, year)  
sets the date only: date, month, year,  
there is no error detection for out-of-range dates, (e.g., April 31)

DS3231\_ReadClock(hour, minute, second, flag, DOW, date, month, year)  
reads the entire clock: hours, minutes, seconds, flag, day of week, date, month, year  
flag = FALSE means a.m.,  
flag = TRUE means p.m.

DS3231\_ReadTime(hour, minute, second, flag)  
reads the time only: hours, minutes, seconds, a.m. or p.m.,  
flag = FALSE means a.m.,  
flag = TRUE means p.m.

DS3231\_ReadDate(date, month, year)  
reads the date only: date, month, year

DS3231\_SetHourMode(12|24)  
sets the hour mode,  
12 = 12-hour  
24 = 24-hour  
any other value defaults to 24-hour mode

DS3231\_ReadHourMode(value)  
returns the current hour mode,

DS3231\_SetSQW(rate)  
sets the square wave output pin mode:  
0 = disable square wave output  
1 = 1 Hz output  
4 = 4096 Hz  
8 = 8192 Hz  
32 = 32768 Hz  
any other value defaults to 1 Hz

DS3231\_EnableSQW  
sets the square wave output pin mode to on

DS3231\_DisableSQW  
sets the square wave output pin mode to off

DS3231\_SetSQWInterruptControl(flag)  
enables the SQW output when flag is TRUE,  
disables the SQW output when flag is FALSE

DS3231\_EnableSQWInterruptControl  
Enables the SQW

DS3231\_DisableSQWInterruptControl  
Disables the SQW

DS3231\_Set32kHz(flag)  
enables the Set32kHz output when flag is TRUE,  
disables the Set32kHz output when flag is FALSE

DS3231\_SetControl (MFP\_Value)  
Sets Control address status to the value of the variable MFP\_Value. The control - rtcc control register is at address 0xOE. Direct access to the control register permits reading and writing of the controls. Set bits usage as specified in the datasheet.

DS3231\_ReadControl  
This function returns the current value of the Control address. See DS3231\_SetControl(for usage.

DS3231\_SetControlStatus (MFP\_Value)  
Sets Control Status address status to the value of the variable MFP\_Value. The control - rtcc control register is at address 0xOE. Direct access to the control register permits reading and writing of the controls. Set bits usage as specified in the datasheet.

DS3231\_ReadControlStatus  
This function returns the current value of the Control Status address. See DS3231\_SetControl(for usage.

DS3231\_SetAlarm1 (Hour, Min, Sec, DOW, Date )  
sets the alarm: hours, minutes, seconds, day of week, date. DOW or Date must BE 0. When DOW is non zero then the alarm if weekly, when Date is non zero then the alarm is monthly.  
There is no error detection for out-of-range dates, (e.g., April 31)  
also sets 24-hour mode.

DS3231\_SetAlarmMask1 (alarmAssertionMatch)  
sets the alarm where Value can be any of the following.

DS3231\_Alarm1Assertion\_EverySecond = 0x0F  
DS3231\_Alarm1Assertion\_Seconds = 0x0E  
DS3231\_Alarm1Assertion\_MinutesSeconds = 0x0C  
DS3231\_Alarm1Assertion\_HoursMinutesSeconds = 0x08  
DS3231\_Alarm1Assertion\_DateHoursMinutesSeconds = 0x00  
DS3231\_Alarm1Assertion\_DayHoursMinutesSeconds = 0x00  
  
A match of these assertions will raise the alarm.

DS3231\_ReadAlarm1 (Hour, Min, Sec, DOW, Date )  
Returns the current settings for a specific alarm.

DS3231\_ClearAlarm1  
Clears a specific alarm after an alarm assertion.

DS3231\_EnableAlarm1Interrupt  
Enables the SQW output to be used to raise an external interrupt

DS3231\_DisableAlarm1Interrupt  
Disables the SQW output to be used to raise an external interrupt

DS3231\_AlarmStatus1  
This is a function. Returns a specific alarm status.  
FALSE means the specific alarm has not met the assertion criteria  
TRUE means the specific alarm has met the assertion criteria

DS3231\_DisableAlarm1  
Disables the alarm.

DS3231\_SetAlarm2 (Hour, Min, DOW, Date )  
sets the alarm: hours, minutes, day of week, date. DOW or Date must BE 0. When DOW is non zero then the alarm if weekly, when Date is non zero then the alarm is monthly.  
There is no error detection for out-of-range dates, (e.g., April 31)  
also sets 24-hour mode.

DS3231\_SetAlarmMask1 (alarmAssertionMatch)  
sets the alarm where Value can be any of the following.

DS3231\_Alarm2Assertion\_EveryMinute = 0x07  
DS3231\_Alarm2Assertion\_Minutes = 0x06  
DS3231\_Alarm2Assertion\_HoursMinutes = 0x04  
DS3231\_Alarm2Assertion\_DateHoursMinutes = 0x00  
DS3231\_Alarm2Assertion\_DayHoursMinutesSeconds = 0x00  
  
A match of these assertions will raise the alarm.

DS3231\_ReadAlarm2 (Hour, Min, DOW, Date )  
Returns the current settings for a specific alarm.

DS3231\_ClearAlarm2  
Clears a specific alarm after an alarm assertion.

DS3231\_EnableAlarm2Interrupt  
Enables the SQW output to be used to raise an external interrupt

DS3231\_DisableAlarm2Interrupt  
Disables the SQW output to be used to raise an external interrupt

DS3231\_AlarmStatus2  
This is a function. Returns a specific alarm status.  
FALSE means the specific alarm has not met the assertion criteria  
TRUE means the specific alarm has met the assertion criteria

DS3231\_DisableAlarm2  
Disables the alarm.

DS3231\_ReadRegister ( in DS\_Value )  
This is a function. Returns the value of the specific register as specified in DS\_Value.

DS3231\_WriteRegister ( in DS\_Value, in DS\_Temp )  
This method set the specific register as specified in DS\_Value to the value specified in DS\_Temp

Version 1.02